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MONBAT SLI PREMIUM EN NP90L5P0_1 100 Ah

[image: ][image: ][image: ][image: ] Mechanical specification
Dimensional group:
L5
ETN reference:
600 044 092 SMF
DIN reference:
60044
DimensionsA in mm (LxWxH):
353x175x190
Cell Layout:
0
Terminal Type:
1

According to EN 50342
Lid
Material
Polypropylene

Cover design
SMF

Colour
Grey


Hold-down
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Layout

Separator
Type
PE


[bookmark: _Hlk25071007]WeightB
Battery weight in kg:
17.10
Acid weight in kg:
6.70
Total battery weight in kg:
23.80


Battery classification as per EN 50342-1
Water consumption
Charge retention
Vibration resistance
Endurance Level
W4
C2
V2
E2

Handles
Material
Polypropylene

Position
Top - on lid

Colour
Grey


Vent caps
Material
Polypropylene

Type
SMF

Colour
Grey


Container
Case
Material
Polypropylene

Bottom hold-down
B13

Colour
Grey

Electrical specification
Voltage:
12V
Capacity C20:                                                     
100 Ah
Cold cranking current:                             
900 A [EN]
Cold cranking current:                             
920 A [SAE]



A. Height taken from bottom of the battery to the highest point on the battery. Heights may vary depending on type of terminal.
B. Weight may vary ±5%.
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